


Can be used for PIT

50MHz =



Disable to prevent unwanted noise from reseting MCU(i.e. Surge)

Set to Enable

